Hazard Communication
The Name of Company (Company) Hazard Communication Program provides information to employees about use, handling and storage of hazardous chemicals.  The full Hazard Communication written program is available from the Company.  This document summarizes the Company’s Hazard Communication program.
Employees have the right:
1. To know how to identify potentially  hazardous chemicals that they may encounter in the workplace;   
2. To know the particular health and safety hazards associated with these chemicals
3. To know how to protect themselves from the effects of these chemicals.
4. For employee’s physician and collective bargaining agent to receive information regarding hazardous chemicals to which an employee may be exposed
5. To not be discharged or receive other disciplinary action due to exercise of employee’s rights under the Hazard Communication law.

Employee should recognize and understand potential  hazards based on:
· Labels on containers
· Information provided  in new SDS (Safety Data Sheet) format
 (
Here is what a uniform label looks like:
Product Identification
 
(
i.e.
, name of product, unique means of identification)
Supplier
/Manufacturer 
 identification:
  
Name
, Address, 
Telephone number
Precautionary Statements
 are related to prevention, response, storage and disposal. ( i.e. “wear respiratory protection” and/or  “wash with soap and water” and/or “store in well ventilated place.”)
Standardized s
ymbols called “Pictograms”
 (see below)
 Note
: 
more than one pictogram may be included, as appropriate.
Signal Words
: there are only two possible words.  (Note: Not all labels will have a signal word  as some chemicals 
do not
 require a signal word)
Danger
: more severe hazard
Warning
: less severe hazard
Hazard Statements
 are specific statements of warning regarding the chemical such as “
Flammable liquid and vapor
” and/or or “
Causes skin irritation
” and/or “
May cause cancer
.”
)Labels on Containers:
[image: ]
Labels on Containers - There are 9 standard Pictograms used globally that cover 30 specific Health Hazards,  Physical Hazards and OSHA Hazard Classifications. 
 (
Irritant
 (skin and eyes)
Skin
 
sensitizer
Acute toxicity (harmful)
Narcotic effects
Respiratory tract 
irrita
nt
Hazardous to ozone layer
)Health Hazards
 (
Acute Toxicity (
fatal 
or toxic
)
)[image: ]   					[image: ]
 (
Carcinogen
Respiratory sensitizer
Reproductive toxicity
Target organ toxicity
Mutagenicity
Aspiration 
Toxicity
)
 (
Skin corrosion
/Burns
Eye 
Damage
Corrosive to metals (
also a 
physical hazard)
)[image: ] 					[image: ] 
Physical Hazards
 (
Flammables
Self -reatives
Pyrophorics
Self-heating
Emits flammable gas
Organic peroxides
) (
Explosives
Self-reactives
Organic Peroxides
)[image: ]					[image: ]  

 (
Oxidizer
s
) (
Gases under Pressure
)[image: ]    					[image: ]
Environment
 (
Aquatic Toxicity
)[image: http://www.oshaguidance.com/wp-content/uploads/2013/04/Aquatic-pollut-red.gif]


Safety Data Sheets (SDS)  
Under revised new Hazard Communication standard, Material Safety Data Sheets (MSDS) are being replaced by Safety Data Sheets (SDS).  All SDS will have a consistent 16-section format.   Each manufacturer or distributor of a chemical provides information about a chemical’s hazards on Safety Data Sheet (SDS).  Note that there is a phase in period, until June 2014, when either the old MSDS or SDS may be used.
SDS are available to all production employees working a show being produced for Viacom through the Viacom/Paramount SDS database maintained by the 3E Company:  

 (
Section 1
 – Identification – identifies chemical and recommended uses.  Contact information for manufacturer/ supplier.
Section 2
 – Hazard(s) identification  - information associated with each identified hazard.
Section 3
 – Composition -Information on Ingredients- impurities and stabilizing additives
Section 4
 – First-aid Measures – initial care before emergency personnel arrive.
Section 5
 – Fire-fighting -Measures in case of fire involving the chemical
Section 6
 – Accidental Release  Measures- How to contain/clean up to spills, leaks, releases.
Section 7
 – Handling and Storage guidance.
Section 8
 – Exposure Controls /Personal Protection- Personal Protective measures to minimize exposure.
Section 9
 – Physical and Chemical Properties
Section 10
 – Stability and Reactivity
Section 11
 – Toxicological Information – Potential health effects, if exposed
Section 12
 – Ecological Information – Potential impacts on physical environment
Section 13
 – Disposal Consideration – Safe handling/disposal information.
Section 14
 – Transport Information- Any special requirements for transporting  the chemical
Section 15
 – Regulatory Information – Any regulations applicable to the specific product.
Section 16
 – Other information including date the SDS was prepared or revised. 
)www.3Eonline.com   
Username = paramount
Password = msds123 or 800-451-8346
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 (
For more information about Hazard Communication, labels or SDSs, please contact 
Who at Company at
)
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SAMPLE LABEL

PRODUCT IDENTIFIER
coDE
Product Name.
SUPPLIER IDENTIFICATION
Company Name,
Street Address
city State
Postal Code Country

Emergency Phone Number
PRECAUTIONARY STATEMENTS

Keep container tightly closed. Store in cool,
well ventilated place that is locked.

Keep aviay from heat/sparks/open flame. No
smoking.

Only use non-sparking tools.

Use explosion-proof electrical equipment.
Take precautionary measure against static
discharge.

Ground and bond container and receiving
equipment.

Do not breathe vapors.

Wear Protective gloves.

Do not eat, drink or smoke when using this
product.

Wash hands thoroughly after handiing.

Dispoae of in accordance with local, regional,

national, international regulations as
specified.

In Case of Fire: use dry chemical (8C) or
Carbon dioxide (CO,) fire extinguisher to

extinguish.

First Aid
If exposed call Poison Center.

I on skin (on hair): Take off immediately any
contaminated clothing. Rinse skin with wiater.

HAZARD PICTOGRAMS

KA

SIGNAL WORD
Danger
HAZARD STATEMENT

Highly flammable fiquid and vapor.
May cause fiver and kidney damage.

SUPPLEMENTAL TNFORMATION
Directions for use
Fill weight: Lot Number

Gross weight: Fill Date:

Expiration Date;
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